                          Sequencer V1.0 (1995)
                          ---------------------

Sequencer V1.0 is a program for the Commodore 64 that is useful for working
with samples, for making own digitized songs from more patterns.

It is very short ($0830-$11FF), therefore you have enough space for samples
($1200-$FFFF)!
That's the reason, why the control is not too comfortable ;-)

It uses NMI timing. SPEED is a low byte of timer (TIMER A)
SPEED -> $DD04                         
#$00  -> $DD05

If speed is set to $90 (high quality), playtime of samples from $1200 to 
$FFFF is about 18 sec.

How to record your own sound:
-----------------------------
This utility supports USER PORT 4-bits samplers connected to data pins C-F
and other data pins H-L connected to GND-0V.

START playing (on the cursor position): 
-----
press '<-'
(to hold '<-' key, fix the adress count.)

STOP playing (& go to CONTROL mode):
----                  -------
press 'RUN/STOP'

Commands in CONTROL mode:
-------------------------
RECORD
------
1.Insert FROM - TO and SPEED on the last line of the screen
  ($90 = fastest 'Hi quality')
  ($FF = slow 'LOW quality')

2.'F2' to start reading samples from USER PORT sampler and playing
  (It is time to start the music and set  the equalizer on your HI-FI)

3.'SPACE' to start recording to memory

COPY
----
1.Insert START - END and HI-byte of NEWSTART (on the SPEED position)
  (on the last line of the screen)

2.'F4'

SAVE
----
1.Insert START - END  (on the last line of the screen)

2.'F6'

EXIT to BASIC
-------------
'F8' (don't use standard RESET)

RESTART
-------
SYS 2096


If you have some questions, ideas, or if you enjoy this program... 
Then please contact me...

Josef Soucek 
(joso@gr.spt.cz)

                              C64 ISN'T DEAD!
