From mmiller3@gac.edu Thu Sep 15 05:52:56 EDT 1994
Article: 122 of comp.binaries.cbm
From: mmiller3@gac.edu
Newsgroups: comp.binaries.cbm
Subject: Internal Stereo SID Modification (Part 00/02) .arc.nu
Date: 14 Sep 1994 14:58:36 GMT
Organization: Gustavus Adolphus College
Lines: 11
Approved: mmiller3@gac.edu (comp.binaries.cbm)
Message-ID: <35732sINNe9g@news.gac.edu>
NNTP-Posting-Host: next-1.gac.edu
Originator: mmiller3@next-1

This file is the description of how to add an internal Stereo SID chip to
your C=64 or 128 computer.  It includes the instructions by Mark A.
Dickenson on how to create the boards necessary for a second stereo chip
and some other information from Q-Link on moving your stereo chip to
locations starting at $D700 (you can choose $DE00 or DF00 without doing
this mod.)  It also includes the modified programs for the StereoPlayer
10.3, Stereo Editor, and another program (for a MIDI editor that I do not
have.)  The file is archived with ARC 250-4, available at ftp.funet.fi.  (I'll .sfx/.sda things from now on, BTW.)

Michael Miller
- mmiller3@gac.edu -


